

**CITY OF EAST PALO ALTO, CALIFORNIA**

**DEPARTMENT OF PUBLIC WORKS – ENGINEERING DIVISION**

**ADDENDUM 5**

**ADDISON AVENUE SAFE ROUTE TO SCHOOL AND GREEN STREET IMPROVEMENTS PROJECT – 22**

**CIP-ST-26**

Date: 3/21/2022

General Information

1. Add Technical Specification Section 110A, “Lime Stabilized Soil” before Section 110. See Addendum 5 Attachment A.
2. Replace Technical Specification Section 110, “Full Depth Reclamation – Cement” with Technical Specification Section 110B, “Full Depth Reclamation – Cement”. See Addendum 5 Attachment B.
3. Replace the Bid Schedule with the Revised Bid Schedule.  Note the quantity of Bid Item No. 31, “Cement (Full-Depth Reclamation – Cement) was revised.   Bid Items No. 69 and 70 were added. See Addendum 5 Attachment C.
4. Add the following paragraphs at the end of Technical Specification Section 100, “Definition of Bid Items”. See Below:

**2.69 Lime Stabilized Soil**.   The contract price paid for “Lime Stabilized Soil” includes full compensation for the required and necessary lime stabilized soil work specified in the Technical Specification and shown on the plans, including asphalt emulsions.

Lime stabilized soil work will be paid by square yard**.** Progress payments will be based on the percentage of lime stabilized soil complete in place.

**2.70 Lime (Lime Stabilized Soil).** The contract price paid for “Lime (Lime Stabilized Soil)” includes full compensation for the required and necessary for lime (lime stabilized soil) work specified in the Technical Specifications and shown on the plans.

Lime (lime stabilized soil) will be paid by ton.  Progress payments will be based on the tons applied.   Contractor shall furnish weight tags to the Engineer daily and shall indicate on the tags the location (lane and which pass) the material was used.

Quantities of lime wasted or disposed of in a manner not specified, or remaining on hand after completion of the work, will not be paid for. Contractor shall maintain records that show the lime utilized and the costs associated with the increase or decrease. If you use a partial load of lime, weigh the truck and the remaining cement on a scale and submit a weighmaster certificate.

Batool Zaro

Batool Zaro

Assistant Engineer

City of East Palo Alto

**ADDENDUM No.5, ACKNOWLEDGMENT**

(To be submitted with the General Construction Contract, Attachment A of RFB)

REQUEST FOR BID – **ADDISON AVENUE SAFE ROUTE TO SCHOOL AND GREEN STREET IMPROVEMENTS PROJECT – 22**

City Project: **CIP-ST-26**

Bidder acknowledges receipt of this addendum, which shall be attached to the bid. Acknowledgement of receipt of this addendum is required in the space provided below. Failure to acknowledge the addendum may subject the bidder to disqualification.

I, , representing have carefully read this addendum, understand it, acknowledge receipt of it and will comply with its terms.

CONTRACTOR SIGNATURE DATE